(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(U1E-V_{SS}-Pad7)")
	(net 2 "Net-(J1-Pin_6)")
	(net 3 "unconnected-(U1-Pad13)")
	(net 4 "Net-(J2-Pin_4)")
	(net 5 "unconnected-(U1-Pad5)")
	(net 6 "unconnected-(U1-Pad12)")
	(net 7 "unconnected-(U1-Pad6)")
	(net 8 "Net-(J2-Pin_1)")
	(net 9 "Net-(J2-Pin_3)")
	(net 10 "unconnected-(U1E-V_{DD}-Pad14)")
	(net 11 "Net-(J2-Pin_2)")
	(net 12 "unconnected-(U2-Pad12)")
	(net 13 "Net-(J1-Pin_5)")
	(net 14 "unconnected-(U2-Pad5)")
	(net 15 "unconnected-(U2-Pad13)")
	(net 16 "Net-(J2-Pin_6)")
	(net 17 "Net-(J2-Pin_5)")
	(net 18 "Net-(J2-Pin_7)")
	(net 19 "unconnected-(U2E-V_{SS}-Pad7)")
	(net 20 "unconnected-(U2E-V_{DD}-Pad14)")
	(net 21 "Net-(J2-Pin_8)")
	(net 22 "unconnected-(U2-Pad6)")
	(net 23 "unconnected-(U3E-V_{SS}-Pad7)")
	(net 24 "unconnected-(U3-Pad5)")
	(net 25 "unconnected-(U3-Pad12)")
	(net 26 "unconnected-(U3-Pad6)")
	(net 27 "unconnected-(U3-Pad13)")
	(net 28 "unconnected-(U3E-V_{DD}-Pad14)")
	(net 29 "Net-(J1-Pin_4)")
	(net 30 "unconnected-(U4E-V_{DD}-Pad14)")
	(net 31 "unconnected-(U4-Pad12)")
	(net 32 "unconnected-(U4E-V_{SS}-Pad7)")
	(net 33 "unconnected-(U4-Pad6)")
	(net 34 "unconnected-(U4-Pad5)")
	(net 35 "unconnected-(U4-Pad13)")
	(net 36 "unconnected-(U5E-V_{DD}-Pad14)")
	(net 37 "unconnected-(U5-Pad6)")
	(net 38 "unconnected-(U5-Pad13)")
	(net 39 "unconnected-(U5-Pad5)")
	(net 40 "unconnected-(U5-Pad12)")
	(net 41 "unconnected-(U5E-V_{SS}-Pad7)")
	(net 42 "unconnected-(U6-Pad5)")
	(net 43 "Net-(J1-Pin_3)")
	(net 44 "unconnected-(U6E-V_{DD}-Pad14)")
	(net 45 "unconnected-(U6E-V_{SS}-Pad7)")
	(net 46 "unconnected-(U6-Pad13)")
	(net 47 "unconnected-(U6-Pad12)")
	(net 48 "unconnected-(U6-Pad6)")
	(net 49 "unconnected-(U7-Pad12)")
	(net 50 "unconnected-(U7E-V_{SS}-Pad7)")
	(net 51 "unconnected-(U7E-V_{DD}-Pad14)")
	(net 52 "unconnected-(U7-Pad6)")
	(footprint "Package_DIP:DIP-14_W7.62mm"
		(layer "F.Cu")
		(uuid "16f527db-4068-484a-abcc-96258692fc12")
		(at 117.272 77.216)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "e2aefeec-35f8-4166-8b56-a7864293f178")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "CD4066BE"
			(at 3.81 17.57 0)
			(layer "F.Fab")
			(uuid "b7133d44-2d24-481a-b9d4-4691f4aa3d41")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "992de840-8ce6-479b-9a03-93263a3e876d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1ddebc25-6321-4443-8c9a-8faaba65348f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, DIP-14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "52ea7687-1668-416e-9c0d-5196e0133a07")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62*")
		(path "/8fa63115-e8f1-4faf-a1cb-7d3041a7ddb8")
		(sheetname "Root")
		(sheetfile "purrChestrion.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da4e399a-d890-4797-83de-464c40e692c8")
		)
		(fp_line
			(start 1.16 16.57)
			(end 6.46 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "03c3a6d3-56ed-4848-a2fe-46dca6e83397")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc7b0245-22c8-4d59-b245-82a77e5c9f9e")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9684db6-53f4-4767-b2e0-94dd77c968b7")
		)
		(fp_line
			(start 6.46 16.57)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eac27610-0ef5-4d37-889e-e7ed86cdb78a")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aaa5290b-f104-4767-87e6-1e12a74541c4")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "093cf403-0142-453a-b287-c33756ba01fd")
		)
		(fp_line
			(start -1.1 16.8)
			(end 8.7 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1fa6e88a-8d4b-4834-b7f1-b8953f3fe3cd")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d907e4d8-0472-4751-9bb7-1514c4b82f3e")
		)
		(fp_line
			(start 8.7 16.8)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "19dd29ec-1edd-448b-949a-3cd27aeda321")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5754c311-6764-49b0-b110-6b2b8d4ce2c3")
		)
		(fp_line
			(start 0.635 16.51)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9300753-39b4-412e-a67f-aa2982ecbddd")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96d32473-571a-45ce-b315-aefe05a08fb0")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d44db862-db46-4167-aab1-c415763fa00b")
		)
		(fp_line
			(start 6.985 16.51)
			(end 0.635 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e3dc98ac-b173-4045-81be-04406a1130ea")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 0)
			(layer "F.Fab")
			(uuid "e53919e6-9f7d-4d24-a7a9-a26509c08229")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_6)")
			(pintype "bidirectional")
			(uuid "bf6f4f6a-612b-41d4-8103-ad4c90c11def")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J2-Pin_4)")
			(pintype "bidirectional")
			(uuid "24b630a8-6081-4919-be6c-a0718bc083ca")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_3)")
			(pintype "bidirectional")
			(uuid "c8474e3d-8aa0-4b35-beb1-00e7c9768518")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_6)")
			(pintype "bidirectional")
			(uuid "1b4bbb9c-a68b-4be2-a111-4b60fc076c99")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(U1-Pad5)")
			(pintype "input")
			(uuid "6bb1a00a-133b-49e1-9dae-adb333a25122")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(U1-Pad6)")
			(pintype "input")
			(uuid "9015f320-8695-45f7-940c-d9f6b86e1b3e")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(U1E-V_{SS}-Pad7)")
			(pinfunction "V_{SS}")
			(pintype "power_in")
			(uuid "11e62383-0448-4d8a-aae1-b8fb0a2540b9")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_6)")
			(pintype "bidirectional")
			(uuid "b9826147-c320-4864-b8ea-59c6f12a64c1")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J2-Pin_2)")
			(pintype "bidirectional")
			(uuid "ea2483d9-9ac5-4a28-9d79-b0c0eafb1a9e")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_1)")
			(pintype "bidirectional")
			(uuid "be1816d1-961f-4f5c-bba6-4dd1227b2f94")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_6)")
			(pintype "bidirectional")
			(uuid "eddc966a-5bb4-43aa-bb4d-dde4665ffb90")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(U1-Pad12)")
			(pintype "input")
			(uuid "7ed01414-4d8c-4116-bde8-939a7204f7ad")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(U1-Pad13)")
			(pintype "input")
			(uuid "22baa78e-83b9-4da1-b403-dc36acba98df")
		)
		(pad "14" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(U1E-V_{DD}-Pad14)")
			(pinfunction "V_{DD}")
			(pintype "power_in")
			(uuid "d0c75505-b476-4982-b76f-a3294a01f0cf")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-14_W7.62mm"
		(layer "F.Cu")
		(uuid "1ef3ee7c-4174-4cf1-8543-b06a30dec42c")
		(at 149.822 77.216)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U4"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "bc730cae-b956-494e-b972-409b6d607416")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "CD4066BE"
			(at 3.81 17.57 0)
			(layer "F.Fab")
			(uuid "e11c4380-ae6c-4294-92da-d409710fff47")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9c60d23d-26cc-4d8f-90d1-a52f0aa85ded")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ea093ed-6528-420e-9fe3-aa999414f5c0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, DIP-14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7df4ca9-8eb2-461c-8e6f-83a25f7ceaa6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62*")
		(path "/488ffea3-5ae1-4626-82cc-79eb28bd8c7c")
		(sheetname "Root")
		(sheetfile "purrChestrion.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f74931c9-e66a-40fc-bfcc-39f362a8451d")
		)
		(fp_line
			(start 1.16 16.57)
			(end 6.46 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d6361c00-6d3a-4d78-9a2d-12be5fbd00c6")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb4e975b-23e2-45e6-8710-bb126e6f531a")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6336f263-6c5f-4be6-af6b-53a5327f32ad")
		)
		(fp_line
			(start 6.46 16.57)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5edaf8cf-7f03-4f13-b5d1-712df50e68c4")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7312a9f0-5098-4743-ba6b-e993cdefa6ce")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "09fb072e-654f-458f-8e21-45704b230839")
		)
		(fp_line
			(start -1.1 16.8)
			(end 8.7 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd6fc91e-d27d-4f9b-ba96-93ce8db4362b")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4d695018-2bf7-49b8-b60c-04adddeec6d0")
		)
		(fp_line
			(start 8.7 16.8)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e6067b3-5f8e-4822-b45f-55dc1c516f47")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e99845e3-7fee-4d21-93d6-34930f67185a")
		)
		(fp_line
			(start 0.635 16.51)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2a24cef-1e8f-484a-9b8a-c597e816771d")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9ebb740-dd73-4e2e-82a2-0adb00c446d8")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98601cd5-b10f-4dcb-b89b-b6d929058f92")
		)
		(fp_line
			(start 6.985 16.51)
			(end 0.635 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9ed3374e-c260-404d-9af4-a2016dfc5076")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 0)
			(layer "F.Fab")
			(uuid "cd645a92-9f49-4777-a1cb-b0fcb7097c5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J1-Pin_4)")
			(pintype "bidirectional")
			(uuid "d894c8bf-6450-4af1-9b9a-90599a3f4c11")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J2-Pin_8)")
			(pintype "bidirectional")
			(uuid "092427f0-c26f-4cb2-bbe2-c463ef499f69")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J2-Pin_7)")
			(pintype "bidirectional")
			(uuid "10a241f8-b383-44de-86ff-a50841a09d1f")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J1-Pin_4)")
			(pintype "bidirectional")
			(uuid "608a4075-7cb0-4fac-a804-635888a47b3a")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(U4-Pad5)")
			(pintype "input")
			(uuid "b3017012-0815-4597-9a39-cd227a49b231")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(U4-Pad6)")
			(pintype "input")
			(uuid "93dc5795-6bdd-419b-8d4d-c2e2897f9be8")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(U4E-V_{SS}-Pad7)")
			(pinfunction "V_{SS}")
			(pintype "power_in")
			(uuid "8234e765-c423-425e-9213-6349589cc18c")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J1-Pin_4)")
			(pintype "bidirectional")
			(uuid "0c93d1ce-b8f9-4b4f-9f25-4677ec803565")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J2-Pin_6)")
			(pintype "bidirectional")
			(uuid "c248fb5c-0cc8-4cdd-baf7-3b7706f66bee")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J2-Pin_5)")
			(pintype "bidirectional")
			(uuid "8b82eb46-cbb7-46e7-a98e-d9d3e3ab4b45")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J1-Pin_4)")
			(pintype "bidirectional")
			(uuid "2834abb8-1b2b-4d9d-b6df-7effa3426fe2")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(U4-Pad12)")
			(pintype "input")
			(uuid "565912c0-48f7-4679-aaed-fa38db6e7874")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(U4-Pad13)")
			(pintype "input")
			(uuid "ebfe87bb-e444-4e1a-948f-38fe88658511")
		)
		(pad "14" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(U4E-V_{DD}-Pad14)")
			(pinfunction "V_{DD}")
			(pintype "power_in")
			(uuid "1f085081-3071-428f-9a3b-65abc49d14fb")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-14_W7.62mm"
		(layer "F.Cu")
		(uuid "439bd438-7639-424b-8ee5-6a29a09c7965")
		(at 128.122 77.216)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U2"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "e430d0ec-2d9b-4a93-916f-567c62943fb4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "CD4066BE"
			(at 3.81 17.57 0)
			(layer "F.Fab")
			(uuid "3e7149f8-012b-4e66-85cd-52c6ffb65230")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "464b2ce6-ebd7-46d3-ab4e-e2af0c9a4a16")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac6c940d-363b-4510-82f0-440ffc2a7a1c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, DIP-14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8e019a17-cf07-4f86-800a-3bf4a1b0e2f2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62*")
		(path "/9d33986c-c00c-442f-9c46-5a2aa7c07eba")
		(sheetname "Root")
		(sheetfile "purrChestrion.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ccf0cb45-af9d-4acf-912e-440daa5cb29e")
		)
		(fp_line
			(start 1.16 16.57)
			(end 6.46 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "05d8eca2-4f8f-4ab0-b09b-e73f8a1f6c6f")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe8bb5a7-76a8-4bd6-a8e2-9fcd123d80a4")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c08067ae-22fe-4e51-9fa9-c5f46050ea1a")
		)
		(fp_line
			(start 6.46 16.57)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0429593b-e993-4590-aa7b-7e2d0bba7fcd")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2345b17f-8758-4d75-81e3-64c6b43d8d2a")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5a39c485-ba53-48db-9437-3aed47b8aed5")
		)
		(fp_line
			(start -1.1 16.8)
			(end 8.7 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d999bf8e-33ec-41a4-a606-9bc849a54225")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3da97b4-6db8-472e-9e0d-2a3105fc8e53")
		)
		(fp_line
			(start 8.7 16.8)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1284669c-a59d-4265-884b-17de517d81fa")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7915deb0-50a4-4398-b8e8-a0304b0c99e8")
		)
		(fp_line
			(start 0.635 16.51)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bfc77133-2bac-491c-a706-3eb5f6d42ba1")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d38e822e-752c-4a64-966b-be3e33e139c2")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "761ed1b2-2c46-47b3-b325-ce655f5466a1")
		)
		(fp_line
			(start 6.985 16.51)
			(end 0.635 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62f77f19-4a1b-4d13-9c0b-155c03acaf59")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 0)
			(layer "F.Fab")
			(uuid "76cc1b2b-6dd6-424e-b388-baad3db13dd0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-Pin_5)")
			(pintype "bidirectional")
			(uuid "ad1892c6-6f45-40b8-ab09-5e3b6b3f8aec")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J2-Pin_8)")
			(pintype "bidirectional")
			(uuid "d646f687-c36d-40d9-96dc-2f419d46d8fa")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J2-Pin_7)")
			(pintype "bidirectional")
			(uuid "ae7e8fba-b64b-4bdf-9d14-e0ba0ee040e0")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-Pin_5)")
			(pintype "bidirectional")
			(uuid "4ab7d317-c016-49e3-843c-bb88d7719ca6")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(U2-Pad5)")
			(pintype "input")
			(uuid "35b9aaea-0db4-42d8-8bb1-1d11b113b627")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(U2-Pad6)")
			(pintype "input")
			(uuid "e6925656-f9eb-4a4a-b6ac-0819cd1115a5")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(U2E-V_{SS}-Pad7)")
			(pinfunction "V_{SS}")
			(pintype "power_in")
			(uuid "cc93ef8d-def4-41ee-b417-bdcbafcd0ff8")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-Pin_5)")
			(pintype "bidirectional")
			(uuid "508d30cb-5ff5-4dcd-b8e6-890e2d2b1613")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J2-Pin_6)")
			(pintype "bidirectional")
			(uuid "a8aa1079-d286-4337-a286-4a9a300803ef")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J2-Pin_5)")
			(pintype "bidirectional")
			(uuid "ab4ba837-0638-4ef5-ad18-e6a394c0fa00")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-Pin_5)")
			(pintype "bidirectional")
			(uuid "3127f8cb-4958-4cef-99a2-125d09463b4b")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(U2-Pad12)")
			(pintype "input")
			(uuid "282edb62-a74c-46dc-ab21-bb5ed5c8cf27")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(U2-Pad13)")
			(pintype "input")
			(uuid "a2d31d1e-e625-4ced-b627-d322060ecb53")
		)
		(pad "14" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(U2E-V_{DD}-Pad14)")
			(pinfunction "V_{DD}")
			(pintype "power_in")
			(uuid "d503e951-0bd4-4020-9811-91cc4613dd7b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-14_W7.62mm"
		(layer "F.Cu")
		(uuid "6964f59c-ac2c-49b1-bf4d-530293d7b859")
		(at 171.522 77.216)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U6"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "9e8836fe-097f-4f49-9837-08c91d3ca659")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "CD4066BE"
			(at 3.81 17.57 0)
			(layer "F.Fab")
			(uuid "d8d8e860-459b-4204-a129-746d0b306293")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "db7cd7c8-8edb-4839-9f87-3f952383e1d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "284594a0-c264-485c-b260-6aaac9a2f76b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, DIP-14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b2ed0374-91c3-4ead-bbce-43e32f63f1fb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62*")
		(path "/e845eeab-9d95-4600-8402-962c0b33e2e6")
		(sheetname "Root")
		(sheetfile "purrChestrion.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d27a686b-b24f-457d-a04c-f69c7e5fa203")
		)
		(fp_line
			(start 1.16 16.57)
			(end 6.46 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f02e74a-d9b1-4723-b1a1-07248e21cf31")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "043fd5e2-af90-40e1-8692-0448d9954da9")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "04c6c65e-bfc6-4d2d-bb6b-b704bbe5cb7a")
		)
		(fp_line
			(start 6.46 16.57)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92abf517-cf1e-4515-a4df-04dac07ec299")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad009da3-157d-460a-b835-5fc45a061111")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fabc83b9-bd69-41f5-bc05-8c8d1d0569bf")
		)
		(fp_line
			(start -1.1 16.8)
			(end 8.7 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dcff5d3b-7c08-4a72-96ec-5c4a4e30e6df")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd0a5302-373d-49f0-8a78-0ea4b211ceef")
		)
		(fp_line
			(start 8.7 16.8)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd176248-e76c-4555-aa87-34047a4cc3d1")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "495c5bda-c305-41b7-800c-5ec0a7b4dd3f")
		)
		(fp_line
			(start 0.635 16.51)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c5e48868-d352-41d9-bf64-ef530a46d673")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb3c7636-ec48-4687-b884-e1f74b0ab433")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95dd170d-6e24-4256-a2cc-59928878dc1c")
		)
		(fp_line
			(start 6.985 16.51)
			(end 0.635 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4abe1e27-29a8-4d3f-965e-a7ccb34ed012")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 0)
			(layer "F.Fab")
			(uuid "eef5fba2-da9e-4d6c-95e2-87f4b96e72fd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1-Pin_3)")
			(pintype "bidirectional")
			(uuid "3d569b10-e836-4846-93af-3115b0206f80")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J2-Pin_8)")
			(pintype "bidirectional")
			(uuid "f01f63d9-ef77-4efa-9eb8-122089cac04a")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J2-Pin_7)")
			(pintype "bidirectional")
			(uuid "aa1ebe8d-aaf6-45db-a5c8-4c40c06de4c6")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1-Pin_3)")
			(pintype "bidirectional")
			(uuid "a06d0c18-ba6d-4993-8c48-2de6e15de792")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(U6-Pad5)")
			(pintype "input")
			(uuid "1fbca735-981a-41b4-8e32-595da49e304c")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(U6-Pad6)")
			(pintype "input")
			(uuid "ea0bc13b-a481-44f7-9030-4959f66c84bb")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(U6E-V_{SS}-Pad7)")
			(pinfunction "V_{SS}")
			(pintype "power_in")
			(uuid "920b0255-147f-4e02-b7b2-4349442f4e25")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1-Pin_3)")
			(pintype "bidirectional")
			(uuid "e971fe40-3dc8-4657-8478-ecac48c43c5b")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J2-Pin_6)")
			(pintype "bidirectional")
			(uuid "6cc01b29-2fee-424c-abe0-7ae21b1d9fcf")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J2-Pin_5)")
			(pintype "bidirectional")
			(uuid "c4608a26-e651-45eb-962d-4cdf7da34857")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1-Pin_3)")
			(pintype "bidirectional")
			(uuid "b451a95d-57c1-4705-8310-eaf2bff74d3a")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(U6-Pad12)")
			(pintype "input")
			(uuid "ceab2272-abc5-4510-8387-09da2cffcd91")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(U6-Pad13)")
			(pintype "input")
			(uuid "c5d085cc-2b20-42d1-9290-a1c7adc6b0b7")
		)
		(pad "14" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(U6E-V_{DD}-Pad14)")
			(pinfunction "V_{DD}")
			(pintype "power_in")
			(uuid "7e18d2cc-22e6-4c66-b79c-ce204855fccb")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-14_W7.62mm"
		(layer "F.Cu")
		(uuid "a88044a5-0e28-48a5-908d-3c699123db2f")
		(at 199.136 76.2)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U7"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "2b6c6aeb-124b-4cd5-83d2-90b9eeb6b226")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "CD4066BE"
			(at 3.81 17.57 0)
			(layer "F.Fab")
			(uuid "910feb4d-c654-4d3b-a36d-c4fa625ded50")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "683acd5b-2866-45b5-8bdf-bc2752d621a7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "188d1bf8-e532-40d5-bdf4-21bc7938101a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, DIP-14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "844442fb-b8c6-4b2d-901c-3f07ba0375e2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62*")
		(path "/83d19aac-af9c-4126-a263-fd4e5e554d9b")
		(sheetname "Root")
		(sheetfile "purrChestrion.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b35a7549-aa3e-472f-bb37-c005df645649")
		)
		(fp_line
			(start 1.16 16.57)
			(end 6.46 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6394bc37-ca36-448c-a395-c58b09ab7a79")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a52f2d6f-5996-478a-ac46-60e003eb15a9")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7965f69-6641-45e0-b158-e9b7fb6dc953")
		)
		(fp_line
			(start 6.46 16.57)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "823b7ef1-1891-4b2c-9c6b-c07ab538591c")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6c63cae-caf5-481a-88c5-e5b83acd4077")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "69d0168b-0cad-417f-9e93-f7e6f9e7a336")
		)
		(fp_line
			(start -1.1 16.8)
			(end 8.7 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4e0782c-096b-4ab4-975a-d82425cb75e6")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "17bf333d-3f8a-4b59-9ede-986da8f1fd83")
		)
		(fp_line
			(start 8.7 16.8)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "031c8e21-7511-4679-b23c-f699519569ec")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb38b38d-d58e-4d7f-bdae-b933eae22904")
		)
		(fp_line
			(start 0.635 16.51)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "899516de-6078-431f-aa7a-f1abb8751523")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c8ab237e-eb01-489b-8de0-f4716f33c604")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7ea8fb13-7d1a-4b1d-95c6-fbf9da62a5b0")
		)
		(fp_line
			(start 6.985 16.51)
			(end 0.635 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4f55b0d-1129-401a-8b56-7c787bde54e3")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 0)
			(layer "F.Fab")
			(uuid "5fe7f990-189d-4efd-8d66-0a8f73929938")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1-Pin_3)")
			(pintype "bidirectional")
			(uuid "0d0bed77-f8de-4859-a7ce-84872bcedfe9")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J2-Pin_4)")
			(pintype "bidirectional")
			(uuid "39265a36-792e-4e0e-a03a-bb82dee046a0")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_3)")
			(pintype "bidirectional")
			(uuid "9f4b1b5e-97b6-43c0-85cf-9853d788b3d2")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1-Pin_3)")
			(pintype "bidirectional")
			(uuid "0f749a12-d030-4bae-85c4-a6feb16b75c8")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J2-Pin_7)")
			(pintype "input")
			(uuid "819c8fe5-16a6-4d1d-b4ed-2ad61b99b345")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(U7-Pad6)")
			(pintype "input")
			(uuid "e433a243-15f7-4426-a69c-39ee311d15e9")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(U7E-V_{SS}-Pad7)")
			(pinfunction "V_{SS}")
			(pintype "power_in")
			(uuid "138d1e1f-32db-4490-96a1-ed5dfdcc0a3e")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1-Pin_3)")
			(pintype "bidirectional")
			(uuid "5d1bf141-9d98-4df3-9244-ab4bbd9c8951")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J2-Pin_2)")
			(pintype "bidirectional")
			(uuid "43bd6d93-e362-4b09-8c96-c1c072c47919")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_1)")
			(pintype "bidirectional")
			(uuid "600389fa-cabd-48f9-9493-c2dfdfc4d932")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1-Pin_3)")
			(pintype "bidirectional")
			(uuid "23278886-f087-4d54-a8f8-ed18ddf2e502")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(U7-Pad12)")
			(pintype "input")
			(uuid "11739ec8-e02f-4b37-b023-13c7a90c3bcc")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J2-Pin_8)")
			(pintype "input")
			(uuid "b782a86b-8335-40bf-9306-40d95f985c00")
		)
		(pad "14" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(U7E-V_{DD}-Pad14)")
			(pinfunction "V_{DD}")
			(pintype "power_in")
			(uuid "3656459d-c7f8-442f-9d5b-aa02b6025bdc")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-14_W7.62mm"
		(layer "F.Cu")
		(uuid "b351d0e5-adbb-4316-ad4d-d678ef247ae2")
		(at 160.672 77.216)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U5"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "9f00f2aa-1272-4a0f-a93c-fb93bd23c0e3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "CD4066BE"
			(at 3.81 17.57 0)
			(layer "F.Fab")
			(uuid "7065ba5e-e9e2-49bb-8183-c43f51594b94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "96ad2ca6-292e-4f2c-b882-eddec4857866")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e9be6f33-2f1c-4519-bc56-6ea20f4ee712")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, DIP-14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "be31b2ec-eea2-4373-bfe8-a724b03f08c9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62*")
		(path "/dbf8001e-65ac-4973-a520-bbb4619ff124")
		(sheetname "Root")
		(sheetfile "purrChestrion.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6c01203c-1593-4bd7-ad03-d4bb56bc7b9d")
		)
		(fp_line
			(start 1.16 16.57)
			(end 6.46 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b3a1672-f923-482b-80e2-ff27987197cf")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf11b7a2-dbc4-4348-b85f-4403bce0243d")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5d7e116d-3cc6-4dc1-ae70-77b39ead148e")
		)
		(fp_line
			(start 6.46 16.57)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8504afcb-bc30-4275-ac9c-324617d7ac41")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "24704041-d571-4114-b784-1ca1a684e13c")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4de7ed49-4f7c-4429-9b62-225b2fc2152e")
		)
		(fp_line
			(start -1.1 16.8)
			(end 8.7 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "784aadab-b5af-4ec3-8fdd-70b65ab5b175")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b141e1cd-2975-4e7f-acba-f1ba5d2584cf")
		)
		(fp_line
			(start 8.7 16.8)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4711a061-d286-439f-9ad4-45fd4d6f9f18")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e1b9db4f-2cc3-4d3a-8e84-50595c89d122")
		)
		(fp_line
			(start 0.635 16.51)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dcec7400-932c-45b7-8edf-5f9caad4a83e")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1389d777-fcb3-44b1-9dc1-967b52dc07e6")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "853dcc32-2d5a-4956-bc2c-cc1d38f239c8")
		)
		(fp_line
			(start 6.985 16.51)
			(end 0.635 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6742c048-51b8-4dd0-8f0c-413f0ae6ecc7")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 0)
			(layer "F.Fab")
			(uuid "fa5a1e06-4d84-4c97-82f2-62d3d62d1d59")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J1-Pin_4)")
			(pintype "bidirectional")
			(uuid "41c01405-68ac-4ee5-8ac2-1fdb54eb58f1")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J2-Pin_4)")
			(pintype "bidirectional")
			(uuid "0de0f186-aa7b-4ada-b1d6-91f297868b83")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_3)")
			(pintype "bidirectional")
			(uuid "611acd29-ce86-432c-af6c-07effd56d47b")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J1-Pin_4)")
			(pintype "bidirectional")
			(uuid "6423aa7b-8b7e-49e4-b51d-70bcba971299")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(U5-Pad5)")
			(pintype "input")
			(uuid "9f8a1456-d019-4745-939a-8930fadec560")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(U5-Pad6)")
			(pintype "input")
			(uuid "4859971d-b6c5-477e-8438-c888291cc155")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(U5E-V_{SS}-Pad7)")
			(pinfunction "V_{SS}")
			(pintype "power_in")
			(uuid "ecb97daf-06fc-44ff-b599-5dff18c5e93c")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J1-Pin_4)")
			(pintype "bidirectional")
			(uuid "e21184b4-f176-47d8-83f2-89bffd93756b")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J2-Pin_2)")
			(pintype "bidirectional")
			(uuid "3464e503-b190-41f8-a607-39ce083bcd04")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_1)")
			(pintype "bidirectional")
			(uuid "8fa50e88-a7eb-4801-b3b7-9477fde7c0e7")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J1-Pin_4)")
			(pintype "bidirectional")
			(uuid "cd7a6ac6-1cd6-4538-a192-2f79a497adf5")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(U5-Pad12)")
			(pintype "input")
			(uuid "ebca7930-26c9-4984-a871-70f65fe00011")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(U5-Pad13)")
			(pintype "input")
			(uuid "7046125a-1437-4e2c-b958-ad0d1e481015")
		)
		(pad "14" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(U5E-V_{DD}-Pad14)")
			(pinfunction "V_{DD}")
			(pintype "power_in")
			(uuid "3b107308-753a-4f07-885f-7489fc3290e4")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-14_W7.62mm"
		(layer "F.Cu")
		(uuid "c5c85293-4434-4e7f-acdd-ec05a70072ec")
		(at 138.972 77.216)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U3"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
			(uuid "55279e11-34ca-4575-b85d-ade28be2a5c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "CD4066BE"
			(at 3.81 17.57 0)
			(layer "F.Fab")
			(uuid "cee19669-3918-471d-b223-125157b9690c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d37db50e-bfe5-4d14-92ef-f5a7629fd4ea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/cd4066b.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b3afbaf9-95b2-421e-b053-322e9f4e8ff7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Quad 20V analog SPST 1:1 switch, DIP-14"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4d97ddc8-39b1-4106-8eff-a6a9878f6a7a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62*")
		(path "/d70529f7-6dfd-40ea-a0fb-d6e374b4620c")
		(sheetname "Root")
		(sheetfile "purrChestrion.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "08e823a3-9b66-4f82-9986-fa3ec397b3bd")
		)
		(fp_line
			(start 1.16 16.57)
			(end 6.46 16.57)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5db20e5a-bd07-44eb-a1bf-09ddc2f78ce9")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d732aaed-fcad-43ef-8dbc-a68fdef6dddd")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "12f3d420-c73b-4147-bc8b-74dd0feb0f3f")
		)
		(fp_line
			(start 6.46 16.57)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6238d50e-df95-4e94-910b-a65af7d22f24")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0a77e5f-5b66-4cf1-894e-e5a8a58d145b")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e58c810b-4a54-487d-bda3-1de205eb8bfe")
		)
		(fp_line
			(start -1.1 16.8)
			(end 8.7 16.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13ca283c-9821-49fb-bb4a-337223b31d56")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e4aeb3ba-236b-4e0f-9be2-4c6de3e5a4c7")
		)
		(fp_line
			(start 8.7 16.8)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "669b7375-940f-4b11-b4f5-553c7a7a5adb")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e20cd9a9-6ab9-49a2-99d3-32806244b6a3")
		)
		(fp_line
			(start 0.635 16.51)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7020430a-9966-404e-b46e-3479542c11b5")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d057cade-2658-437b-bf16-b81d71153e20")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd6e77ae-c2e8-4c73-9229-5dc4bb9918a4")
		)
		(fp_line
			(start 6.985 16.51)
			(end 0.635 16.51)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3158d61f-3f98-4a7e-97a8-963ac10b07c8")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 0)
			(layer "F.Fab")
			(uuid "0ac352c1-d1fb-46c8-8109-a1f49499b5f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-Pin_5)")
			(pintype "bidirectional")
			(uuid "8bdee945-4625-4b03-b110-361cb2e4ca26")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J2-Pin_4)")
			(pintype "bidirectional")
			(uuid "481db9d3-520a-488d-9644-ed98afe1ff05")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_3)")
			(pintype "bidirectional")
			(uuid "d03c9765-6e71-4fb8-9915-ddeaa0ba02f1")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-Pin_5)")
			(pintype "bidirectional")
			(uuid "7486c02d-185c-47fd-b834-d8f64378001a")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(U3-Pad5)")
			(pintype "input")
			(uuid "40d8b87f-34a8-4edd-a944-edf6f656aee8")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(U3-Pad6)")
			(pintype "input")
			(uuid "802b6c7f-403d-46cf-a6e3-200cd786d5ad")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(U3E-V_{SS}-Pad7)")
			(pinfunction "V_{SS}")
			(pintype "power_in")
			(uuid "392199ae-f280-4b8c-82b3-2b5270be3db9")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-Pin_5)")
			(pintype "bidirectional")
			(uuid "b46ecf88-7494-44ef-bfb4-0928717ca89a")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J2-Pin_2)")
			(pintype "bidirectional")
			(uuid "da9fd8d4-2a70-4711-9ab3-4cff41eb182f")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_1)")
			(pintype "bidirectional")
			(uuid "679deb1a-0c35-44e1-96db-b0284d9a9c36")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-Pin_5)")
			(pintype "bidirectional")
			(uuid "6ddf87db-a218-456f-afa4-a72f32c41cf0")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(U3-Pad12)")
			(pintype "input")
			(uuid "6d460ca1-568e-484c-af31-d0caae5406ea")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(U3-Pad13)")
			(pintype "input")
			(uuid "b26fd15d-067e-4698-ae4c-5463d798a4fa")
		)
		(pad "14" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(U3E-V_{DD}-Pad14)")
			(pinfunction "V_{DD}")
			(pintype "power_in")
			(uuid "c2a534b5-ff34-4cad-9698-24498702035e")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
)
